**Part 6 Attachments**

Part 6 contains information that will help the contractor develop a suitable design and construct without hindrance.

Example attachments are:  
 – Schematic sketches showing work locations  
 – Catalog cuts  
 – Record drawings  
 – Environmental Hazards Assessment Reports (asbestos, lead based paint, paint, radon, PCB, Low-Level Radioactive components, , animal droppings, mold and spores, waste characterization, chlordane)  
– Photographs, including general site and specific site problems, such as storm water erosion  
 – Soil boring logs, geotechnical reports  
 – Base Exterior Architecture Plan (BEAP)/Installation Appearance Plan (IAP)